**Wobbler kit onto trolley mounting**

**Parts list**

**4 x Nuts & bolts 4 x Short legs**

**A group of black metal brackets

Description automatically generated4 x M10 x 25mm bolts  
4 x nylon locking nuts**

**A group of bolts and nuts

Description automatically generated**

**2 wheel trolley Wobbler kit**

**A black and red metal cart on grass

Description automatically generatedA black metal object with wires on grass

Description automatically generated**

**Step 1**

**Assemble the trolley**

**Attach the axle and fasten with the 2 x m10 x 40mm bolt with nylon locking nut.**

**A black and red wheel with red wheels

Description automatically generated**

**Slide the 2 x wheels onto the axle and fasten the m22 nylon nut onto the axle end thread.**

**A black and red metal cart

Description automatically generated**

**Step 2**

**A black metal object with a black metal object on top of it

Description automatically generatedA black machine on top of a box

Description automatically generatedAttach the wobbler kit short legs**

**A black metal object with wires and screws on grass

Description automatically generated**

**Attach the 4 x short legs onto the wobbler kit and nip the clamp bolt hand tight for now.**

**Step 3**

**Attach the wobbler kit to the trolley**

**A black and red cart on grass

Description automatically generatedA black metal object with red wheels on grass

Description automatically generated**

**A black metal object with red wheels

Description automatically generatedMount the wobbler kit onto the trolley and align the pre-drilled holes. You may need to loosen the clamp bolts to align the holes.**

**Once you locate 1 x bolt per foot, tighten each foot nut and bolt, then tighen each clamp bolt holding the leg on. Do not over tighten.**